**Customized press seal**

with segmented ring technology

Article Code: HRD SGi b40

GTIN: -

Brand: Hauff-Technik

For sealing cables in core drills or wall sleeves. Split design for sealing new installed cables or cables that have already been installed. The number of cables and cable diameters can be selected on an individual basis.

Dimensions: Sealing width: 40 mm; Press plates: 5 mm; Available for core drills/wall sleeves Ø: 50 - 200 mm

Material: Press plates, screws, nuts and washers: rust-free stainless steel V2A (AISI 304L) or V4A (AISI 316L); Rubber: EDPM or NBR

Application range: Waterproof concrete stress class 1 and 2

Tightness: gastight and watertight; Radon-proof

Features: tailor-made to meet requirements; Segmented ring technology for adjustment on-site to pipe diameters

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de